| Earth Observation Mission CFI Software DataHandling Software User Manual |

Public Member Functions | Public Attributes

# EECFI::PolarMotionParams Class Reference

Polar motion parameters.. More...

List of all members.

## Public Member Functions
| PolarMotionParams ()
| Default constructor.
| PolarMotionParams (double x1, double y1)
| Constructor with parameters.
## Public Attributes
double | x
| x-axis is in the direction of the IERS Reference Meridian (IRM).
double | y
| y-axis is in the direction 90 degrees West longitude.

## Detailed Description

Polar motion parameters..

## Constructor & Destructor Documentation

EECFI::PolarMotionParams::PolarMotionParams | ( |  | ) | `[inline]`

Default constructor.

EECFI::PolarMotionParams::PolarMotionParams | ( | double | x1,
|  | double | y1 |
| ) |  |  | `[inline]`

Constructor with parameters.

## Member Data Documentation

double EECFI::PolarMotionParams::x

x-axis is in the direction of the IERS Reference Meridian (IRM).

double EECFI::PolarMotionParams::y

y-axis is in the direction 90 degrees West longitude.