| Earth Observation Mission CFI Software Lib Software User Manual |

Public Member Functions | Public Attributes

# EECFI::LaunchInertialFrameConfig Class Reference

Data structure defining launch inertial frame config. More...

List of all members.

## Public Member Functions
* | LaunchInertialFrameConfig ()
| Default constructor.
## Public Attributes
long | enabledFlag
| Flag indicating the time is initialized with eogs*/.
double | longitude
| End of Giro Setting (longitude)*/.
double | utcTime

## Detailed Description

Data structure defining launch inertial frame config.

## Constructor & Destructor Documentation

* EECFI::LaunchInertialFrameConfig::LaunchInertialFrameConfig | ( |  | ) | `[inline]`

Default constructor.

## Member Data Documentation

long EECFI::LaunchInertialFrameConfig::enabledFlag

Flag indicating the time is initialized with eogs*/.

Referenced by EECFI::TimeCorrelation::getData(), and EECFI::TimeCorrelation::setData().

double EECFI::LaunchInertialFrameConfig::longitude

End of Giro Setting (longitude)*/.

Referenced by EECFI::TimeCorrelation::getData(), and EECFI::TimeCorrelation::setData().

double EECFI::LaunchInertialFrameConfig::utcTime

End of Giro Setting (UTC time)

Referenced by EECFI::TimeCorrelation::getData(), and EECFI::TimeCorrelation::setData().