| Earth Observation Mission CFI Software DataHandling Software User Manual |

Public Member Functions | Public Attributes

# EECFI::BulbTable Class Reference

Class to store the data for one entry read from the IERS bulletin. More...

List of all members.

## Public Member Functions
| BulbTable ()
| Empty constructor.
| BulbTable (double dayUtc, double diffUt1Utc, double diffUt1Tai)
| Constructor with parameters.
## Public Attributes
double | day
| MJD UTC time.
double | ut1Utc
| Difference between UT1 and UTC.
double | ut1Tai
| Difference between UT1 and TAI.

## Detailed Description

Class to store the data for one entry read from the IERS bulletin.

## Constructor & Destructor Documentation

EECFI::BulbTable::BulbTable | ( |  | ) | `[inline]`

Empty constructor.

EECFI::BulbTable::BulbTable | ( | double | dayUtc,
|  | double | diffUt1Utc,
|  | double | diffUt1Tai |
| ) |  |  | `[inline]`

Constructor with parameters.

## Member Data Documentation

double EECFI::BulbTable::day

MJD UTC time.

double EECFI::BulbTable::ut1Tai

Difference between UT1 and TAI.

double EECFI::BulbTable::ut1Utc

Difference between UT1 and UTC.