| Earth Observation Mission CFI Software DataHandling Software User Manual |

Public Member Functions | Public Attributes

# EECFI::IersBulletinArec Class Reference

Class to store the data for one entry read from the IERS bulletin A. More...

List of all members.

## Public Member Functions
| IersBulletinArec ()
| Default constructor.
| IersBulletinArec (double dayUtc, double diffUt1Utc, double diffUt1Tai, PolarMotionParams polarMotion)
| Constructor with parameters.
## Public Attributes
double | day
| MJD UTC time.
double | ut1Utc
| Difference between UT1 and UTC.
double | ut1Tai
| Difference between UT1 and TAI.
PolarMotionParams | polarMotionParams
| Polar motion parameters.

## Detailed Description

Class to store the data for one entry read from the IERS bulletin A.

## Constructor & Destructor Documentation

EECFI::IersBulletinArec::IersBulletinArec | ( |  | ) | `[inline]`

Default constructor.

EECFI::IersBulletinArec::IersBulletinArec | ( | double | dayUtc,
|  | double | diffUt1Utc,
|  | double | diffUt1Tai,
|  | PolarMotionParams | polarMotion |
| ) |  |  | `[inline]`

Constructor with parameters.

## Member Data Documentation

double EECFI::IersBulletinArec::day

MJD UTC time.

PolarMotionParams EECFI::IersBulletinArec::polarMotionParams

Polar motion parameters.

double EECFI::IersBulletinArec::ut1Tai

Difference between UT1 and TAI.

double EECFI::IersBulletinArec::ut1Utc

Difference between UT1 and UTC.