| Earth Observation Mission CFI Software Visibility Software User Manual |

Public Attributes

# EECFI::MultiStationsExtraInfo Class Reference

Additional information to visibility segments computed for multiple stations. More...

Inheritance diagram for EECFI::MultiStationsExtraInfo:

List of all members.

## Public Attributes
long | numberOfStations
| Number of station from which the satellite is visible during the segment (dummy if extraInfoFlag == false).
vector< long > | stationsInSegment
| Indexes of the stations from which the satellite is visible during the segment (dummy if extraInfoFlag == false). It is not filled for Swath::multiStationsVisTime.
vector< ANXTime > | multiZdop
| Zero doppler orbit time (dummy if extraInfoFlag == false).
vector< string > | stationNamesInSegment
| Name of the station (only for Swath::stationVisTimeCompute).
vector< double > | utcTime
| UTC time for zero doppler (only for Swath::stationVisTimeCompute).

## Detailed Description

Additional information to visibility segments computed for multiple stations.

## Member Data Documentation

vector<ANXTime> EECFI::MultiStationsExtraInfo::multiZdop

Zero doppler orbit time (dummy if extraInfoFlag == false).

long EECFI::MultiStationsExtraInfo::numberOfStations

Number of station from which the satellite is visible during the segment (dummy if extraInfoFlag == false).

vector<string> EECFI::MultiStationsExtraInfo::stationNamesInSegment

Name of the station (only for Swath::stationVisTimeCompute).

vector<long> EECFI::MultiStationsExtraInfo::stationsInSegment

Indexes of the stations from which the satellite is visible during the segment (dummy if extraInfoFlag == false). It is not filled for Swath::multiStationsVisTime.

vector<double> EECFI::MultiStationsExtraInfo::utcTime

UTC time for zero doppler (only for Swath::stationVisTimeCompute).