| Earth Observation Mission CFI Software DataHandling Software User Manual for JAVA |

Public Member Functions | Public Attributes

# EECFI.PolarMotionParams Class Reference

Polar motion parameters. More...

List of all members.

## Public Member Functions
| PolarMotionParams ()
| Constructor.
| PolarMotionParams (double x1, double y1)
| Constructor with parameters.
| PolarMotionParams (PolarMotionParams pm)
| Copy constructor.
## Public Attributes
double | x
| x-axis is in the direction of the IERS Reference Meridian (IRM).
double | y
| y-axis is in the direction 90 degrees West longitude

## Detailed Description

Polar motion parameters.

## Constructor & Destructor Documentation

EECFI.PolarMotionParams.PolarMotionParams | ( |  | ) |

Constructor.

EECFI.PolarMotionParams.PolarMotionParams | ( | double | x1,
|  | double | y1 |
| ) |  |  |

Constructor with parameters.

EECFI.PolarMotionParams.PolarMotionParams | ( | PolarMotionParams | pm | ) |

Copy constructor.

## Member Data Documentation

double EECFI.PolarMotionParams.x

x-axis is in the direction of the IERS Reference Meridian (IRM).

double EECFI.PolarMotionParams.y

y-axis is in the direction 90 degrees West longitude