| Earth Observation Mission CFI Software Pointing Software User Manual for JAVA |

Public Member Functions | Public Attributes

# EECFI.InstrumentData Class Reference

Instrument input data. More...

List of all members.

## Public Member Functions
| InstrumentData ()
| Empty constructor.
| InstrumentData (long typ, AzimuthElevationList azElList, AzimuthElevationStrip azElStrip, AzimuthElevationGrid azElGrid, double freq)
| Constructor with parameters.
## Public Attributes
long | type
| See AzElTypeEnum.
AzimuthElevationList | azimuthElevationList
| List of azimuth and elevation points.
AzimuthElevationStrip | azimuthElevationStrip
| Strip of points with fixed azimuth.
AzimuthElevationGrid | azimuthElevationGrid
| Grid of azimuth/elevation points.
double | signalFrequency
| Frequency of signal.

## Detailed Description

Instrument input data.

## Constructor & Destructor Documentation

EECFI.InstrumentData.InstrumentData | ( |  | ) |

Empty constructor.

EECFI.InstrumentData.InstrumentData | ( | long | typ,
|  | AzimuthElevationList | azElList,
|  | AzimuthElevationStrip | azElStrip,
|  | AzimuthElevationGrid | azElGrid,
|  | double | freq |
| ) |  |  |

Constructor with parameters.

## Member Data Documentation

AzimuthElevationGrid EECFI.InstrumentData.azimuthElevationGrid

Grid of azimuth/elevation points.

AzimuthElevationList EECFI.InstrumentData.azimuthElevationList

List of azimuth and elevation points.

AzimuthElevationStrip EECFI.InstrumentData.azimuthElevationStrip

Strip of points with fixed azimuth.

double EECFI.InstrumentData.signalFrequency

Frequency of signal.

long EECFI.InstrumentData.type

See AzElTypeEnum.