| Earth Observation Mission CFI Software DataHandling Software User Manual for JAVA |

Variables

# DemGdemV2DataSourceEnum

DEM Data Source Types for GDEM V2. More...

## Variables
static long | EECFI::EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_NO_SOURCE_FILE = -1
| QA value contain the number of scene-based DEMs contributing to the final GDEM value for each 30m pixel (stack number)*/.
static long | EECFI::EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_SRTM3_V3 = 0
| SRTM3 V3: Posting: 3 arc seconds Coverage: north 60deg to south 56deg Only about 90 % tiles of SRTM V3 are void filled*/.
static long | EECFI::EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_SRTM3_V2 = 1
| SRTM3 V2: Posting: 3 arc seconds Coverage: north 60deg to south 56*/.
static long | EECFI::EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_NED = 2
| NED: Posting: 1 arc second Coverage: Conterminous U.S.*/.
static long | EECFI::EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_CDED = 3
| CDED: Posting: 3 arc seconds for latitude; 3, 6 and 12 arc seconds for longitude, depending on latitude Coverage: all Canada territory */.
static long | EECFI::EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_ALASKA_DEM = 4
| ALASKA_DEM: Posting: 2 arc seconds Coverage: all Alaska territory*/.

## Detailed Description

DEM Data Source Types for GDEM V2.

## Variable Documentation

long EECFI.EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_ALASKA_DEM = 4`[static, inherited]`

ALASKA_DEM: Posting: 2 arc seconds Coverage: all Alaska territory*/.

long EECFI.EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_CDED = 3`[static, inherited]`

CDED: Posting: 3 arc seconds for latitude; 3, 6 and 12 arc seconds for longitude, depending on latitude Coverage: all Canada territory */.

long EECFI.EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_NED = 2`[static, inherited]`

NED: Posting: 1 arc second Coverage: Conterminous U.S.*/.

long EECFI.EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_NO_SOURCE_FILE = -1`[static, inherited]`

QA value contain the number of scene-based DEMs contributing to the final GDEM value for each 30m pixel (stack number)*/.

long EECFI.EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_SRTM3_V2 = 1`[static, inherited]`

SRTM3 V2: Posting: 3 arc seconds Coverage: north 60deg to south 56*/.

long EECFI.EnumDataHandling.XDCFI_DEM_GDEM_SOURCE_SRTM3_V3 = 0`[static, inherited]`

SRTM3 V3: Posting: 3 arc seconds Coverage: north 60deg to south 56deg Only about 90 % tiles of SRTM V3 are void filled*/.