| Earth Observation Mission CFI Software Pointing Software User Manual for JAVA |

Public Member Functions | Public Attributes

# EECFI.GenDemAltFromEllipsoidInputs Class Reference

DEM set selection. More...

List of all members.

## Public Member Functions
| GenDemAltFromEllipsoidInputs ()
| Empty Class constructor.
| GenDemAltFromEllipsoidInputs (long type, double minLon, double maxLon, double minLat, double maxLat, long verb)
| Constructor with parameters.
## Public Attributes
long | setType
| DEM set selected (DemSetEnum).
double | lonMin
| Minimum longitude of interval.
double | lonMax
| Maximum longitude of interval.
double | latMin
| Minimum latitude of interval.
double | latMax
| Maximum latitude of interval.
long | verbose
| If 0, no output will be printed. If > 0, a message will be printed every verbose points.

## Detailed Description

DEM set selection.

## Constructor & Destructor Documentation

EECFI.GenDemAltFromEllipsoidInputs.GenDemAltFromEllipsoidInputs | ( |  | ) |

Empty Class constructor.

EECFI.GenDemAltFromEllipsoidInputs.GenDemAltFromEllipsoidInputs | ( | long | type,
|  | double | minLon,
|  | double | maxLon,
|  | double | minLat,
|  | double | maxLat,
|  | long | verb |
| ) |  |  |

Constructor with parameters.

## Member Data Documentation

double EECFI.GenDemAltFromEllipsoidInputs.latMax

Maximum latitude of interval.

double EECFI.GenDemAltFromEllipsoidInputs.latMin

Minimum latitude of interval.

double EECFI.GenDemAltFromEllipsoidInputs.lonMax

Maximum longitude of interval.

double EECFI.GenDemAltFromEllipsoidInputs.lonMin

Minimum longitude of interval.

long EECFI.GenDemAltFromEllipsoidInputs.setType

DEM set selected (DemSetEnum).

long EECFI.GenDemAltFromEllipsoidInputs.verbose

If 0, no output will be printed. If > 0, a message will be printed every verbose points.