| Earth Observation Mission CFI Software DataHandling Software User Manual for JAVA |

Variables

# DemAce2DataSourceEnum

DEM Data Source Types for ACE2: 9secs and 30secs. More...

## Variables
static final long | EECFI::EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM0 = 0
| Pure SRTM (above 60 deg N pure GLOBE data, below 60S pure ACE [original] data).
static final long | EECFI::EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM1 = 1
| SRTM voids filled by interpolation and/or altimeter data.
static final long | EECFI::EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM2 = 2
| SRTM data warped using the ERS-1 Geodetic Mission.
static final long | EECFI::EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM3 = 3
| SRTM data warped using EnviSat & ERS-2 data.
static final long | EECFI::EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM_LAKE = 4
| Mean lake level data derived from Altimetry.
static final long | EECFI::EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM_GLOBE = 5
| GLOBE/ACE data warped using combined altimetry (only above 60 deg N).
static final long | EECFI::EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM_ALT = 6
| Pure altimetry data (derived from ERS-1 Geodetic Mission ERS-2 and EnviSat data using Delaunay Triangulation and Bilinear interpolation).

## Detailed Description

DEM Data Source Types for ACE2: 9secs and 30secs.

## Variable Documentation

final long EECFI.EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM0 = 0`[static, inherited]`

Pure SRTM (above 60 deg N pure GLOBE data, below 60S pure ACE [original] data).

final long EECFI.EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM1 = 1`[static, inherited]`

SRTM voids filled by interpolation and/or altimeter data.

final long EECFI.EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM2 = 2`[static, inherited]`

SRTM data warped using the ERS-1 Geodetic Mission.

final long EECFI.EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM3 = 3`[static, inherited]`

SRTM data warped using EnviSat & ERS-2 data.

final long EECFI.EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM_ALT = 6`[static, inherited]`

Pure altimetry data (derived from ERS-1 Geodetic Mission ERS-2 and EnviSat data using Delaunay Triangulation and Bilinear interpolation).

final long EECFI.EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM_GLOBE = 5`[static, inherited]`

GLOBE/ACE data warped using combined altimetry (only above 60 deg N).

final long EECFI.EnumDataHandling.XDCFI_DEM_ACE2_SOURCE_SRTM_LAKE = 4`[static, inherited]`

Mean lake level data derived from Altimetry.