| Earth Observation Mission CFI Software Lib Software User Manual for JAVA |

Public Member Functions | Public Attributes

# EECFI.GeoDistance Class Reference

Data structure for geodetic distance. More...

List of all members.

## Public Member Functions
| GeoDistance ()
| Empty constructor.
| GeoDistance (double dist, double az1, double az2)
| Constructor with parameters.
## Public Attributes
double | distance
| Geodesic distance between the two input points (EF CS).
double | az1to2
| Azimuth of the geodesic line from point 1 to point 2 (Topocentric CS).
double | az2to1
| Azimuth of the geodesic line from point 2 to point 1 (Topocentric CS). Note that az2to1 = az1_to_2 + 180 approx.

## Detailed Description

Data structure for geodetic distance.

## Constructor & Destructor Documentation

EECFI.GeoDistance.GeoDistance | ( |  | ) |

Empty constructor.

EECFI.GeoDistance.GeoDistance | ( | double | dist,
|  | double | az1,
|  | double | az2 |
| ) |  |  |

Constructor with parameters.

## Member Data Documentation

double EECFI.GeoDistance.az1to2

Azimuth of the geodesic line from point 1 to point 2 (Topocentric CS).

double EECFI.GeoDistance.az2to1

Azimuth of the geodesic line from point 2 to point 1 (Topocentric CS). Note that az2to1 = az1_to_2 + 180 approx.

double EECFI.GeoDistance.distance

Geodesic distance between the two input points (EF CS).